Locking Gas Cap Instructions

Installation
1. Insert the key into the gas cap lock. 
2. Turn the key counterclockwise.
Place the cap onto the filler neck.
Make sure the tabs on the bottom of the cap line up with the slots on the filler neck. 
3. Turn the cap clockwise until it is tight.
You should feel the cap fully seat into the closed position. 
4. Turn the key clockwise back to the locked position, then remove the key. 
5. Once locked, the cap will spin freely.
This is normal and prevents the cap from being removed without the key. 

Removal
1. Insert the key into the gas cap lock. 
2. Hold the cap and turn the key counterclockwise.
This unlocks the internal mechanism so the cap can be removed. 
3. With the key still turned, rotate the cap counterclockwise until it stops. 
4. Lift the cap off the filler neck.
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